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Eliminator II Tail Light Instructions 

CV4826/CV4826B/CV4827/CV4827B/
CV4828/CV4828B/CV4829/CV4829B/
                                                                      CV4830/CV4830B/CV4831/CV4831B

                                     CV4832/CV4832B
                                                                       Fits: 86-02 FXST, 86-05 FXWG

NOTE: It may be necessary to notch the license plate for the license plate light wiring.

USE ALLEN WRENCH TO HOLD SETSCREW WHILE TIGHTENING LOCK NUT
We will not warranty if the setscrew goes through face of the frame.

96 & UP Models:

1. Before installation remove seat and unplug taillight wiring harness.

2. Remove stock tail light, rear turn signals and associated wiring from rear fender. (refer to H-D service manual for removal)
3. Install new light assembly and route wires thru rear fender clips, plug in new wire harness 
Note: Ensure wires will not hit rear tire
PRE-96 Models:

1. Before installation remove seat and unplug taillight wiring harness.

2. Remove stock tail light, rear turn signals and associated wiring from rear fender. (refer to H-D service manual for removal)
3. Install new light assembly and route wires thru rear fender clips 
4. Locate bike rear light and turn signal wire harness.

5. Cut rear tail light and turn signal wires approximately 3 inches from plug.

6. The 8 pin connector pigtail MUST be spiced or “Hard-wired” in to the Main Bike rear light wire harness.

NOTE: a test light must be used to determine what wire corresponds with the Cycle Visions Color Code as below.

CYCLE VISIONS Wiring Color Code

Black…………Ground

Red……..Brake Light

Blue…..Run light

Brown….Right turn

Purple…Left Turn

Orange… Acc/Fender tip light

DO NOT INSTALL THIS UNIT WITHOUT APPLYING LOCKTITE

TO EVERY SCREW, NUT OR BOLT!

Our Warranty Policy

Cycle Visions’ obligation under “Our Warranty Policy” is limited to one (1) year from date of purchase to repair or replacement of the defective item (s).  Chrome, polished, powder-coated, anodized finishes, or electrical parts are limited to thirty (30) day from date of purchase.

This warranty will be void on all products that show evidence of misapplication, improper installation, abuse, lack of proper maintenance, negligence, or alteration from their original design.

The consumer will be responsible for removing from the vehicle any defective item (s), transportation costs prepaid and for reinstallation upon return by Cycle Visions.  The loss of use of the product, loss of time, inconvenience, commercial loss or consequential damages is not covered.  Cycle Visions reserves the right to change the design of any product without assuming any obligation to modify any product previously manufactured.  Warranty returns of Cycle Visions products are few because of our high quality products.

Carefully inspect all parts…. If you find that your parts arrived in damaged conditional all original packaging material (box and other materials) must be saved to make a proper damage claim within seven (7) days.  You must be able to present the damaged boxes and materials to the freight carrier to verify your claim.  The user shall assume all legal, personal, injury risk and liability and all other obligations, duties and risks associated therewith

See our other products on the web!                                                                                                                                                                                                       Cycle Visions(
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