
The Heating Thermostat BYC03 USER  MANUAL
General Information

· The heating thermostat  BYC03 using the latest SCM control technology, high reliability and strong anti-interference. All the way to high-current relay contacts, electric heating temperature control or automatic thermostat controlled area;
· [image: image1.png]


Large-screen displays, user-friendly design, simple and practical.
· The shell is made of flame-retardant materials, safe and reliable.
· Input voltage: 220V + / -10%
· Set the temperature: 5 ℃ -35 ℃
· Measuring temperature: 0 ℃ -40 ℃
· Relay contact capacity: 16A/250VAC
· Shell material: flame retardant PC
Turning On / Off
· Power on / off: Press [image: image17.emf]

 key can turn on or off the thermostat.
· When off the display shows the current room temperature;
Setting the timer
· Press [image: image2.emf]

 to enter the timer settings. Press [image: image3.png]


 or [image: image4.png]


 to carry out regular time set the timing for the start-up," TIMER ON "," TIMER OFF "Sleep timer. 
· On the timer mode, the display alternately displays the timing time and measure temperature.
· Set timed shutdown can be done by remote control settings.
Setting temperature for times of the day

· Temperature setting: Press [image: image5.png]


 or [image: image6.png]


 key, the screen displays "SET" and can set the temperature for need.
Lock the keyboard
· Press the M key for 3 seconds to lock the keyboard, the screen display ---. 
· In the locked state, press the M key 3 seconds to unlock.
Temperature calibration

· When the thermostat on OFF state, Press the [image: image7.png]


 to turn on and show “byc”, please press [image: image8.emf]

 Key in two seconds to enter the system menu, the first item of the system menu for temperature calibration can be used [image: image9.png]


 or [image: image10.png]


 adjust the correction value after the input screen will display calibrated temperature value. Button [image: image11.emf]

 to proceed to the second temperature units set, C-Celsius and F-Fahrenheit, it can be switch by  [image: image12.png]


 or [image: image13.png]


  key. Then press the [image: image14.emf]

 key to exit the system menu.
Points for attention 

· When setting if the hard plastic wires, please bend the right angle first

· The temperature of using the thermostat: 0°C~45°C

· Please do the connection according the wire diagram

· Please don’t pressure to the LCD, and no broking to the thermostat.
· No cashing, no bumping and no comedown.
· Please don’t let the back shell deformation. Don’t fall down the mud.
Malfunction disposal    Statement: only professional technical personnel can amend in the products of our company.

	Malfunction
	Disposal

	Boot-strap error
	1.Check L,N power and the wiring connection；

2.Check the switch button；

3.Change the control board, or change the power supply board;

	No output with

right display
	1.Power control panels and connecting cable may be damaged；

2.Change the control board and then change the power plate

	Remote failure
	1.Check whether there is a remote battery power；

2.Change the remote

	temperature display abnormal
	The temperature has not been calibrated.


Warranty service  

· 18 months warranty service is from date of purchase.

· Note: The Service Center shall not be liable for any LCD scratch, break or damage to wire, back board, shell power supply board due to loading or installation.

Sale support

· The products of our company may enjoy life-long service in accordance with regulations; the company will make a certain charge to the service out of the warranty period or product quality.

Packaging Annex           Manual 1pcs and Bolt 2pcs
Product Dimensions                unit: mm
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