New TFT LCD MONITOR Surveillance CCTV Camera Tester Detector Test 12V Handheld GH4



Features:
1.Built-in Li battery; Video-in terminal and DC power supply
2.It is easy to hold and do not need complicated equipment that hinders the inspecting and repairing
3.High image resolution monitor enable to show clear image Long work time
4.Equips with Li-ion battery of high capability
5.Each 4 hours recharge durables 6~7 work hours
6.Humanized design of appearance
7.Hand-hold design for professionals
8.Easy operation without taking off gloves speeds your works
9.Support DC power for camera
10.It's convenient for user to check camera condition and correct direction of camera, so to make installation and repairing easier 

Specifications:
1.Display: 2.5"TFT Color LCD
2.Image Resolution: 960x240 pixels
3.Video In: Video in x 1 (BNC Connector)
4.Power out: DC power out x 1(Support CCD camera of power source/Max electric currency 400mA)
5.System Format: NTSC/PAL
6.Status Indicator: 2LED(Power IND = Green / Charging IND =Red)
7.Interface: OSD power
8.Power Source: Built-in rechargeable Lithium battery : 3.7V 1400mA
9.Power Source: External power :DC 5V 1.0A Adapter
10.Dimension: 85mm(L) X 31mm(W) X 190mm(H)

Package included:
1 x Camera Detector
1 x Transformer
1 x CCD power cord
1 x 3.7V 1400mA li-ion battery
1 x Lanyard
1 x Users manual
