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THIS IS A TRADITIONAL ROLL DESIGNED TO LIMIT THE MOTION OF THE HELMET. MORE SECURE THAN LACE-ON ROLLS; INSERTING FOUR SCREWS MOUNT THE NECK ROLL.
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ROLL


INSTALLATION


INSTRUCTIONS





1. ALIGN THE FOUR BRASS EYELETS OF THE ROLL ON TOP OF THE SHOULDER PAD SHELL.





2. MARK THE HOLES THROUGH THE GROMMETS, AND DRILL HOLES (IF NECESSARY) IN SHOULDER PAD.





3. INSERT THE SCREW ASSEMBLIES AS SHOWN.








