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USER MANUAL

NECK&Shoulder MASSAGER

ITEM NO.: MSF005
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IMPORTANT SAFEGUARDS

When using massager products, basic precautions should always be followed, to reduce the risk of being hurt, including the following:

· Always unplug the appliance from the electrical outlet immediately after using and before cleaning.

· DO NOT reach for an appliance that has fallen into water. Unplug it immediately.

· DO NOT use while bathing or in the shower.

· DO NOT place or store appliance where it can fall or be pulled into a tub or sink.

· DO NOT place into or drop into water or other liquid.

· NEVER use pins or other metallic fasteners with this appliance.

· Keep dry – DO NOT operate in a wet or moist condition.

· An appliance should never be left unattended when plugged in. Unplug from outlet when not in use and before putting on or taking off parts and attachments.

· Close supervision is necessary when this appliance is used by, on or near children, invalids or disabled persons.

· Use this appliance only for its intended use as described in this manual. ONLY use attachments provided with the unit.

· NEVER operate this appliance if it has a damaged cord or plug, if it’s not working properly, if it has been dropped or damaged, or dropped into water.

· Keep cord away from heated surfaces.

· NEVER use while sleeping or fall asleep while using the massager.

· NEVER drop or insert any object into any opening.

· DO NOT operate where aerosol (spray) products are being used or where oxygenise being administered.

· DO NOT operate under a blanket or pillow. Excessive heating can occur and cause fire, electric shock or injury to persons.

· DO NOT carry this appliance by power cord or use cord as handle.

· To disconnect, turn all controls to the “Off” position, then remove plug from outlet.

· This appliance is designed for personal, non-professional use only.

· DO NOT use outdoors.

· DO NOT use on an infant or invalid or on a sleeping or unconscious person.

· DO NOT use on sensitive skin or on a person with poor blood circulation.

CAUTION-PLEASE READ ALL INSTRUCTIONS CAREFULLY BEFORE OPERATING

· DO NOT crush. Avoid sharp folds.
· Consult your doctor prior to using this product, if you are pregnant, if you have pacemaker or any concerns regarding your health.

· Never leave this appliance unattended, especially if children are present.

· Never leave the appliance when it is in operation.

· DO NOT use this product for more than 15 minutes at a time.

· Extensive use could lead to the product’s excessive heating and shorter life. Should this occur, discontinue use and allow the unit to cool before operating.

· Never use this product directly on swollen or inflamed areas or skin eruptions.

· This product is a non-professional appliance designed to provide soothing massage for back and legs.
· It must only be supplied at safety extra low voltage corresponding to the marking on the appliance          
· DO NOT use this product as a substitute for medical attention.

· DO NOT use this product before bed. The massage has a stimulating effect and may delay sleep.

· NEVER use this product while in bed.

· This product should NEVER be used by any individual suffering from any physical condition that would limit the user’s capacity to operate the controls or who has sensory deficiencies in the lower half of their body.
· It must only be supplied at safety extra low voltage corresponding to the marking on the appliance

· Children or invalids without adult supervision should not use this unit.

· In order to reduce the inrush current on the impact of this product, Please shut down after waiting 30 seconds before turning on power, And to avoid frequent start, so you can extend the life of the product.
	Description
	Neck Massager

	Model no
	MSF005
	Power
	24W

	Voltage:
	DC12 V / AC100-240 V- DC12V adaptor


POWER ADAPTOR

This unit is equipped with a power adaptors: 100-240volt adaptor for home use, connect the proper adaptor as shown below:

_ DO NOT use any other adaptor that is not equipped with the unit, may cause serious loss,
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INSTRUCTION FOR USE

Plug the 100-240 volt adaptor into a 100-240 volt AC outlet and plug the receptacle into 
the input jack that located along the side of the massager.
Handhold Belt

This massager incorporates a convenient hanger belt design , it will allow you to adjust the massage

Intensity or fasten the massage position by pull it. 


Location of Parts

1. Massage Device

2. Control panel

3. Hand Belt

Control Panel

  Heat : Massage with heat

  Power: Start/stop massaging

  Direction: Change the rotating direction of massage heads

Operation Manual

1. Make sure the power has been properly connected.

2. Press POWER button to start shiatsu massaging.

3. When massage is on, press HEAT button to on/off heating function.

4. When massage is on,press Direction button to change the rotating direction of massage heads

5. Stop Massage:

Rated working time is 15 mins, Press POWER button to stop massaging during 15mins or it will auto shut off after 15 mins.

Notice:

The massager will be auto shut off After 15 mins of massage program, we suggest leaving the machine for cooling to avoid over-heating or destroy the electrical parts and motors inside. There is a anti-overheating device builted in machine.

ONE YEAR LIMITED WARRANTY
We guarantee this product free from defects in material and workmanship for a period of one years from the date of original purchase, except as noted below.

This product warrant does not cover damage cause by :misuse or abuse;accident; the attachment of any unauthorized accessory; alteration to the product; or any other conditions what-so-ever that are beyond the control of original agent. 

This warranty is effective only if the product is purchased and operated in your own country. A product that requires modification or adaption to enable it to operate in any country other than the country for which it was designed, manufactured, approved and / or authorized, or repair of products damaged by these modifications is not covered under warranty. We shall not be responsible for any type of incidental. Consequential or special damages. All implied warranties. Including but no limited to those implied warranties of fitness and merchantability, are limited in the total duration of one year from the original purchase date.







plug this receptacle end into the 100-240 volt power outlet.





Plug the receptacle end into the power outlet of the massager





�





�











�








1
2

