                W34 Smart watch User Manual
Thank you for choosing our product!

To have a comprehensive understanding and using this device, to know all the features and simple operation method, please read this manual first.

The functions on the user manual may be little different with physical, please make the final products as the standard.

The typing errors in this manual and discrepancies will be timely updated with the latest products. If we have updates, this manual will be subject to change without notice. Our company reserves the right of final interpretation.

Charging instructions: standard 5PIN USB charging port, support computer USB or mobile phone 5V standard charger, about 70 minutes can be full of power.
Watch connects to Phone, download the App “Fundo” in the Phone at first, reference following 2 methods:

1) Android/iOS Phone: Scan following QR code image by browsers or by any Scanner to Download “Fundo”.
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2) Android Phone: search and download “Fundo” app from Google Play;

iOS phone: search and download “Fundo” app from Apps Store;

After installation, turn on cellphone Bluetooth and Fundo App, confirm the notification enable, tap “More” at right bottom corner, enter add device, search “Watch_LE” device and tap connect, then you are succeeding connected the Bluetooth 4.0; 

Next go to watch side Bluetooth-searching Bluetooth-select turn on Bluetooth-tap your cellphone name in the list-confirm the connection at your cellphone end. Then you are succeeding connected Bluetooth 3.0; 

Only when Bluetooth 3.0 & 4.0 both connected the watch can be abled full performance, slide down the watch you will see the Bluetooth icon, green color at upper means Bluetooth 3.0 is connected, Blue color at bottom means Bluetooth 4.0 is connected. 

How to setting notification: into phone’s Settings-App Management, find “ Fundo”-Authority Management, open all allow.

Into Notifications- find “Fundo”, open all allow. Into “ Fundo”- “Application push”, select all allow.

As the Bluetooth protocol is different between all the mobile phone brands. Sometimes the Bluetooth connection will be instability between mobile phone and smart watch. Please restart the Bluetooth, then try to connect again, or restore factory settings. If appear system halted, please long press power button about 10 seconds to restart watch. 

※ Operation Guide
The home button: long press to switch watch, short press to return to the standby interface, when watch crashed, long press 10 seconds to restart .
TP gestures: slide right/left/up to enter the main menu, after entering each function, slip from left to right for return, slip from right to left for confirmation
Watch face switch: long press the screen, there will be a dial choice, tap confirm.

Main menu: Slide right/left to enter, slide left to next page. Slide right to return. 

Main function

Calling

Dial: Bluetooth call via cellphone, talk at the watch end.

Phonebook: Sync all the contacts in the cellphone, max is 400 contacts.
Call logs: Sync all the calls history in the cellphone.

SMS: Sync all the messages in the cellphone (Not support iOS phone yet).

Bluetooth: Search the device you want connect, or disconnect the devices.
Pedometer: check the steps you walked during the day, calories burn and walk distance. Everyday 0 o’clock all the data will be saved automatically and reset to 0. Slide up enter option; status, on and off; history, it can check 7 days local records; Goal, set a target for everyday steps; put into all your information, such as Gender, Height, Weight etc. for more accurate measure your steps data.
Sleep monitor：The smart watch will turn on it automatically from 9p.m to 9a.m. It records your sleep duration and quality, help you adjust a better rest time, improve sleep quality. Slide up enter options; Status, On and Off; History, check out deep sleep and light sleep; instruction.
Heart rate monitor: wear the watch tightly with your wrist, best position would be upper of the hand-wrist, around 20 seconds it will shows the real time heart rate data, slide down menu into history, mode includes single measure and continuous measure; and instruction. Generally speaking normal value is 60-90 times/min.

ECG: adopt optical heart rate and ECG combine technology, about 30 seconds can show the data, after test will appear ToAPP, means ECG data save to phone “Fundo”.   
Sedentary: Set a long-time reminder of sit, remind you have a stand when time up.
Anti-lost: click “find phone”, connected phone will be ringing warning, after find the phone, tap “End” of the phone to stop the alarm, it works both watch and Apps sides.
Alarm: can setting 5 alarm, long press can cancel alarm.

Stopwatch: Single timing, tap the left icon to start timing, and tap to pause, tap again for cumulative time.

Calculator: 

Calendar:

Bluetooth Setting: Turn on/off the Bluetooth in watch.
Clock: clock type, there are 4 standby watch faces to choose; 
Face: have two standby face can be choose.
Gesture: support for call turnover mute, alarm flip over mute, gesture wake up system (ie It is to raise the hand to automatically light screen), shake to answer the call; 

Sound: you can select the caller profile, select Ringtones, select notification ringtones; 
Volume: adjustable volume for media, ring tones, notifications, etc.; 
Power-saving mode: turn watch on to enter clock mode, other functions are turned off; display, access to adjustable screen brightness and backlight off duration; 
About: you can view the watch model and software version.
Data transmission: mobile phone to download Fundo App, after the connection is successful, either steps data, heart rate data, the sleep quality, multiple sports can be transmitted to the mobile end. 

Warranty
1. If it appears quality problems caused by manufacturing, materials, design within one year（since the day of purchase）, battery and cable within 6 months. we will offer free warranty. Premise is using normally and correctly.

2. About the fault caused by the user’s personal reasons, we don't offer free warranty, as follows:

1). Disassemble or refit the product.

2). Caused by immodesty drop 

3). All artificial damage or misuse (such as: make water into the host, the external force shatter, scratch damage of peripheral components, etc.), all these are beyond the scope of the warranty.

3. When ask for free warranty, you must provide a warranty card with the seal of purchase place and purchase date.

4. If you met problems during use, please contact the shop customer service which you bought from.

5. Please make the final products as the standard.
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