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SMK-Link Electronics Corporation

3601-B Calle Tecate, Camarillo, CA  93012

Phone (805) 987-6662, Fax (805) 987-6665

www.interlinkelec.com
Product Announcement Information Sheet
	Product Name
	Bluetooth Calculator Keypad

	Model Number
	VP6270

	Part Number
	KUX0102-1001F

	UPC Code
	7 15262 06270 2  [image: image2.emf]

	Dimensions/Weight per Single Package
	204mm x 125mm x 50mm; 287g
8.0” x 4.9” x 2.0”; 10 oz

	Dimensions/Weight per Shipping Carton
	333mm x 149mm x 257mm; 1.8 kg
13.1” x 5.9” x 10.1”; 4.0 lb

	Quantities per Shipping Carton
	6 units

	Suggested Retail Price
	US$59.99

	Availability
	May 19, 2008
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PRODUCT DESCRIPTIONS

Short Description – 25 Words

· The VP6270 Bluetooth Calculator Keypad is an innovative 2-in-1 device that is not only a wireless Bluetooth ten-key for Mac and Windows, but also a standalone calculator. 

Standard Description – 50 Words

· Interlink Electronics’ VP6270 Bluetooth Calculator Keypad increases productivity for notebook users.  This wireless numeric keypad doubles as a ten-key for spreadsheets and data entry and as a stand alone calculator.  The VP6270 features an LCD display, Bluetooth wireless up to 33 feet and works with both Mac and PC.

Long Description – 100 Words

· Interlink Electronics’ VP6270 Bluetooth Calculator Keypad increases productivity for notebook users.  This wireless numeric keypad doubles as a ten-key for spreadsheets and data entry and as a stand alone calculator.  The VP6270 features an LCD display, Bluetooth wireless up to 33 feet and works with both Mac and PC. Calculations computed on the keypad can be sent directly into a spreadsheet just like you typed them.  Cut the cord and go wireless. For computers with Bluetooth built in, there is no need for any dongle or cord. For those without, it works perfectly with Interlink Electronics’ Nano Bluetooth Dongle.
FEATURES AND BENEFITS

Built-in Fully Functional Calculator
· The embedded off-line calculator function means one less device to clutter the desktop and less weight in your computer carrying case.
· The built-in 12 digit LCD display provides visualization to the calculation functions.

· The one-touch SEND key ensures the calculated result is correctly transcribed to the spreadsheet without having to rekey-in the numbers, therefore eliminating potential data entry errors.

Latest Bluetooth Technology for the Ultimate Wireless Experience
· The VP6270 is designed with Bluetooth v2.0 EDR (Enhanced Data Rate) technology offering 3 times the data transmission speed.
· Featuring Bluetooth Class 2 for up to 33 feet of wireless data transmission range.
· Simple process to connect to the Bluetooth host computer; no need to install software.  Once connection is established, it stays connected to the host even after power-off.

· No more cables to clutter the desktop with the wireless freedom Bluetooth provides; and no need to carry, and to plug in, a proprietary dongle for the keypad.
The Ultimate 2-in-1 Bluetooth Tool for Spreadsheet Numeric Data Entry
· No need to install drivers, the VP6270 is the only numeric keypad that’s 100% compatible with both Windows and Mac OS, thus allowing Mac users to switch between the 2 operating systems without losing any functions.  (Exception: does not support French OS due to different numeric key layout.)
· The VP6270 is one of the most practical accessories for Bluetooth notebook computers.  As the majority of notebook PC’s do not offer a keypad for their built-in keyboard, numeric data entry becomes a challenge, especially for finance and accounting professionals.  The VP6270 not only provides an effortless way to enter numbers, it also replaces the traditional calculator so that only one device is needed.  The VP6270 Bluetooth Calculator Keypad is truly the most desirable companion to a Bluetooth notebook computer.
Additional Opportunities with SMK-Link Bluetooth Products
Opportunity to Upgrade Your PC to Bluetooth
· SMK-Link also offers a Nano Bluetooth Class 2 Dongle, which is the most compact Bluetooth adapter available today.  Priced at $39.99, the Interlink VP6494 Nano Bluetooth Class 2 Dongle upgrades any PC to Bluetooth, providing up to 33 feet of wireless connectivity between your system and your Bluetooth devices.

Opportunity to Upgrade Your Notebook Accessories to Bluetooth
· Other Interlink-branded Bluetooth devices offered by SMK-Link, working seamlessly with the VP6494 Nano Bluetooth Class 2 Dongle, are the VP6150 and VP6151 Rechargeable Bluetooth Notebook Mouse in addition to the new VP6270 Bluetooth Calculator Keypad.  Also scheduled for June, 2008 launch is the VP4570 Bluetooth Stopwatch Presenter with Laser Pointer.
SPECIFICATIONS

Product Specifications

· Bluetooth v2.0 with EDR (Enhanced Data Rate)
· Class 2 supports up to 33 feet/10 meters operating range

· Computer keypad with built-in calculator function and 12-digit LCD display

· 19-key computer keypad:
· Numeric keys: 00, 0, 1, 2, 3, 4, 5, 6, 7, 8, 9

· Arithmetic Operators: “+”, “-“, “*”, “/”

· Operation keys: Wake/CE/AC, Back Space, Enter, “.”

· 6 calculator function keys:

· Set decimal place, MRC, M+, M-, +/-, %

· 2 hot keys:
· Mode switch, Send number

· Low-profile membrane key constructions

· Power source: 2 x AAA batteries

· Hardware requirement: Bluetooth-enabled system (via built-in native Bluetooth or external adapter)

· OS compatibility: Windows 2000, XP, Vista

      Mac OS X or later

Note: French OS is not supported due to different numeric key layout.

· Dimensions: 6.4” x 3.7” x 1.2” / 162 x 93 x 30mm
· Weight: 6.5-oz / 185g

· BQB, FCC and CE certified

Package Contents
· Bluetooth calculator keypad
· 2 x AAA batteries
· User’s manual
Warranty

· 12 months limited warranty
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